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Air leakage has always been the main problem of Dunnage bags. After years of experience International Dunnage has come up with a super tough bladder bag to prevent the air leakages caused by pinholes, minor scratches or cuts. The new multilayer bladder bags have been tested under tough conditions and show no signs of leakage. They are manufactured 100% by fully automated state of art machine without the touch of a hand. 














 TOUGH BAG





NEW





For lighter duty bags 2 layers and for heavy duty bags 4 layers of film are used on each side. The outer layers protect the inner layers from external damages. 








International Dunnage Combo valve is designed for fast fill and discharge, which is spring loaded and can be used for every level. They are reusable and easy to handle. Combo valve has passed the compression test under severe climate conditions and they are 100% leak tested during production.











International Dunnage Combo inflator tips are designed to perfectly fit Combo valves and can resist high pressures. They can be easily snapped on to the valve by pressing against a wall. They are designed to be used with both International Dunnage Mini Jet Flow and Monster air guns, however other air guns may also be used connecting by an air hose. Combo Inflator Tips are made out of hard plastic materials. Aluminum version is also available for heavy duty use.





NEW





New vacuum system for packaging/palettizing of airbags increasing capacity of paletts by 30%, resulting in significant reduction of required storage space for your stock.
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